# Menu 18 − Application Menu 1

Mode: Open‑Loop

General option module application menus

Menus 18 and 20 are general application menus that can be used by one of the option modules fitted to the drive. These menus are customisable and the following RAM is provided to be shared between the 2 menus.

| 1 | 8 | 16 | 32
Volatile | 0 | 0 | 9 | 10
User save | 20 | 0 | 20 | 0
Power-down save | 0 | 0 | 1 | 4

If no option modules provide customisation tables for these menus then the drive provides the customisation tables to give the following parameters.

Parameter | 18.001 Application Menu 1 Power-down Save Integer
--- | ---
Short description | General power-down save integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit Power Down Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.002 Application Menu 1 Read-only Integer 2
--- | ---
Short description | General read-only integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 18.003 Application Menu 1 Read-only Integer 3
--- | ---
Short description | General read-only integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 18.004 Application Menu 1 Read-only Integer 4
--- | ---
Short description | General read-only integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 18.005 Application Menu 1 Read-only Integer 5
--- | ---
Short description | General read-only integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 18.006 Application Menu 1 Read-only Integer 6
--- | ---
Short description | General read-only integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 18.007 Application Menu 1 Read-only Integer 7
--- | ---
Short description | General read-only integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 18.008 Application Menu 1 Read-only Integer 8
--- | ---
Short description | General read-only integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 18.009 Application Menu 1 Read-only Integer 9
--- | ---
Short description | General read-only integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 18.010 Application Menu 1 Read-only Integer 10
--- | ---
Short description | General read-only integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default |  | Units |
Type | 16 Bit Volatile | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RO, PR, ND, NC

Parameter | 18.011 Application Menu 1 Read-write Integer 11
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.012 Application Menu 1 Read-write Integer 12
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.013 Application Menu 1 Read-write Integer 13
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.014 Application Menu 1 Read-write Integer 14
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.015 Application Menu 1 Read-write Integer 15
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.016 Application Menu 1 Read-write Integer 16
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.017 Application Menu 1 Read-write Integer 17
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.018 Application Menu 1 Read-write Integer 18
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.019 Application Menu 1 Read-write Integer 19
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.020 Application Menu 1 Read-write Integer 20
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.021 Application Menu 1 Read-write Integer 21
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.022 Application Menu 1 Read-write Integer 22
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.023 Application Menu 1 Read-write Integer 23
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.024 Application Menu 1 Read-write Integer 24
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.025 Application Menu 1 Read-write Integer 25
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.026 Application Menu 1 Read-write Integer 26
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.027 Application Menu 1 Read-write Integer 27
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.028 Application Menu 1 Read-write Integer 28
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.029 Application Menu 1 Read-write Integer 29
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.030 Application Menu 1 Read-write Integer 30
--- | ---
Short description | General read-write integer application parameter
Mode | Open‑Loop
Minimum | -32768 | Maximum | 32767
Default | 0 | Units |
Type | 16 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.031 Application Menu 1 Read-write bit 31
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.032 Application Menu 1 Read-write bit 32
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.033 Application Menu 1 Read-write bit 33
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.034 Application Menu 1 Read-write bit 34
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.035 Application Menu 1 Read-write bit 35
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.036 Application Menu 1 Read-write bit 36
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.037 Application Menu 1 Read-write bit 37
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.038 Application Menu 1 Read-write bit 38
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.039 Application Menu 1 Read-write bit 39
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.040 Application Menu 1 Read-write bit 40
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.041 Application Menu 1 Read-write bit 41
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.042 Application Menu 1 Read-write bit 42
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.043 Application Menu 1 Read-write bit 43
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.044 Application Menu 1 Read-write bit 44
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.045 Application Menu 1 Read-write bit 45
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.046 Application Menu 1 Read-write bit 46
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.047 Application Menu 1 Read-write bit 47
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.048 Application Menu 1 Read-write bit 48
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.049 Application Menu 1 Read-write bit 49
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.050 Application Menu 1 Read-write bit 50
--- | ---
Short description | General read-write bit application parameter
Mode | Open‑Loop
Minimum | 0 | Maximum | 1
Default | 0 | Units |
Type | 1 Bit User Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.051 Application Menu 1 Power-down Save Long Integer 51
--- | ---
Short description | General power-down save long integer application parameter
Mode | Open‑Loop
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit Power Down Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.052 Application Menu 1 Power-down Save Long Integer 52
--- | ---
Short description | General power-down save long integer application parameter
Mode | Open‑Loop
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit Power Down Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.053 Application Menu 1 Power-down Save Long Integer 53
--- | ---
Short description | General power-down save long integer application parameter
Mode | Open‑Loop
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit Power Down Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW

Parameter | 18.054 Application Menu 1 Power-down Save Long Integer 54
--- | ---
Short description | General power-down save long integer application parameter
Mode | Open‑Loop
Minimum | -2147483648 | Maximum | 2147483647
Default | 0 | Units |
Type | 32 Bit Power Down Save | Update Rate | N/A
Display Format | Standard | Decimal Places | 0
Coding | RW