# Menu 11 Single Line Descriptions − Miscellaneous

Mode: Open‑Loop

Parameter | Range | Default | Type
--- | --- | --- | ---
11.018 | Status Mode Parameter 1 | 0.000 to 30.999 | 2.001 | RW | Num |  |  | PT | US
11.019 | Status Mode Parameter 2 | 0.000 to 30.999 | 4.020 | RW | Num |  |  | PT | US
11.020 | Reset Serial Communications | Off (0) or On (1) |  | RW | Bit | ND | NC |  |
11.021 | Customer defined scaling | 0.000 to 10.000 | 1.000 | RW | Num |  |  |  | US
11.022 | Active Parameter At Power‑up | 0.000 to 0.095 | 0.010 | RW | Num |  |  | PT | US
11.023 | Serial Address | 1 to 247 | 1 | RW | Num |  |  |  | US
11.024 | Serial Mode | 8.2NP (0), 8.1NP (1), 8.1EP (2), 8.1OP (3), 8.2NP E (4), 8.1NP E (5), 8.1EP E (6), 8.1OP E (7), 7.1EP (8), 7.1OP (9), 7.1EP E (10), 7.1OP E (11) | 8.2NP (0) | RW | Txt |  |  |  | US
11.025 | Serial Baud Rate | 600 (1), 1200 (2), 2400 (3), 4800 (4), 9600 (5), 19200 (6), 38400 (7), 57600 (8), 76800 (9), 115200 (10) Baud | 19200 (6) Baud | RW | Txt |  |  |  | US
11.026 | Minimum Comms Transmit Delay | 0 to 250 ms | 2 ms | RW | Num |  |  |  | US
11.027 | Silent Period | 0 to 250 ms | 0 ms | RW | Num |  |  |  | US
11.028 | Drive Derivative | 0 to 255 |  | RO | Num | ND | NC | PT |
11.029 | Software Version | 0 to 99999999 |  | RO | Num | ND | NC | PT |
11.030 | User Security Code | 0 to 9999 |  | RW | Num | ND |  | PT | US
11.031 | User Drive Mode | OPEn.LP (1), RFC‑A (2) |  | RW | Txt | ND | NC | PT |
11.032 | Maximum Heavy Duty Rating | 0.00 to 9999.99 A |  | RO | Num | ND | NC | PT |
11.033 | Drive Rated Voltage | 110V (0), 200V (1), 400V (2), 575V (3), 690V (4) |  | RO | Txt | ND | NC | PT |
11.034 | Drive Configuration | AV (0), AI (1), AV.Pr (2), AI.Pr (3), Preset (4), Pad (5), Pad.Ref (6), E.Pot (7), Torque (8), Pid (9) | AV (0) | RW | Txt |  |  | PT | US
11.035 | Power Software Version | 0 to 99999999 |  | RO | Num | ND | NC | PT |
11.036 | NV Media Card File Previously Loaded | 0 to 999 | 0 | RO | Num |  | NC | PT |
11.037 | NV Media Card File Number | 0 to 999 | 0 | RW | Num |  |  |  |
11.038 | NV Media Card File Type | None (0), OPEn.LP (1), RFC‑A (2), UPrG (5) |  | RO | Txt | ND | NC | PT |
11.039 | NV Media Card File Version | 0 to 9999 |  | RO | Num | ND | NC | PT |
11.042 | Parameter Cloning | None (0), Read (1), Prog (2), Auto (3), Boot (4) | None (0) | RW | Txt |  | NC |  | US
11.043 | Load Defaults | None (0), Std (1), US (2) | None (0) | RW | Txt |  | NC |  |
11.044 | User Security Status | LEVEL.1 (0), LEVEL.2 (1), ALL (2), Status (3), no.acc (4) |  | RW | Txt | ND |  | PT |
11.045 | Select Motor 2 Parameters | 1 (0), 2 (1) | 1 (0) | RW | Txt |  |  |  | US
11.046 | Defaults Previously Loaded | 0 to 2000 |  | RO | Num | ND | NC | PT | US
11.047 | Onboard User Program: Enable | Stop (0), Run (1) | Run (1) | RW | Txt |  |  |  | US
11.048 | Onboard User Program: Status | -2147483648 to 2147483647 |  | RO | Num | ND | NC | PT |
11.049 | Onboard User Program: Programming Events | 0 to 65535 |  | RO | Num | ND | NC | PT |
11.050 | Onboard User Program: FreewheelingTasks Per Second | 0 to 65535 |  | RO | Num | ND | NC | PT |
11.051 | Onboard User Program: Clock Task Time Used | 0.0 to 100.0 % |  | RO | Num | ND | NC | PT |
11.052 | Serial Number LS | 000000 to 999999 |  | RO | Num | ND | NC | PT |
11.053 | Serial Number MS | 0 to 999999 |  | RO | Num | ND | NC | PT |
11.054 | Drive Date Code | 0000 to 9999 |  | RO | Num | ND | NC | PT |
11.055 | Onboard User Program: Clock Task Schedule Rate | 0 to 262128 ms |  | RO | Num | ND | NC | PT |
11.060 | Maximum Rated Current | 0.000 to 999.999 A |  | RO | Num | ND | NC | PT |
11.061 | Full Scale Current Kc | 0.000 to 999.999 A |  | RO | Num | ND | NC | PT |
11.063 | Product Type | 0 to 255 |  | RO | Num | ND | NC | PT |
11.064 | Product Identifier Characters | 1127428144 to 2147483647 |  | RO | Num | ND | NC | PT |
11.065 | Frame size and voltage code | 000 to 999 |  | RO | Num | ND | NC | PT |
11.066 | Power Stage Identifier | 0 to 255 |  | RO | Num | ND | NC | PT |
11.067 | Control Board Identifier | 0 to 255 |  | RO | Num | ND | NC | PT |
11.068 | Drive current rating | 00000 to 32767 |  | RO | Num | ND | NC | PT |
11.070 | Core Parameter Database Version | 0.00 to 99.99 |  | RO | Num | ND | NC | PT |
11.072 | NV Media Card Create Special File | 0 to 1 | 0 | RW | Num |  | NC |  |
11.073 | NV Card Type Fitted | None (0), Res (1), Sd.Card (2) |  | RO | Txt | ND | NC | PT |
11.075 | NV Media Card Read‑only Flag | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
11.076 | NV Media Card Warning Suppression Flag | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
11.077 | NV Media Card File Required Version | 0 to 9999 |  | RW | Num | ND | NC | PT |
11.079 | Drive Name Characters 1‑4 | -2147483648 to 2147483647 | 757935405 | RW | Num |  |  | PT | US
11.080 | Drive Name Characters 5‑8 | -2147483648 to 2147483647 | 757935405 | RW | Num |  |  | PT | US
11.081 | Drive Name Characters 9‑12 | -2147483648 to 2147483647 | 757935405 | RW | Num |  |  | PT | US
11.082 | Drive Name Characters 13‑16 | -2147483648 to 2147483647 | 757935405 | RW | Num |  |  | PT | US
11.084 | Drive Mode | OPEn.LP (1), RFC‑A (2) |  | RO | Txt | ND | NC | PT | US
11.085 | Security Status | None (0), r.only.A (1), Status (2), no.acc (3) |  | RO | Txt | ND | NC | PT | PS
11.086 | Menu Access Status | LEVEL.1 (0), LEVEL.2 (1), ALL (2) |  | RO | Txt | ND | NC | PT | PS
11.091 | Additional Identifier Characters 1 | -2147483648 to 2147483647 |  | RO | Num | ND | NC | PT |
11.092 | Additional Identifier Characters 2 | -2147483648 to 2147483647 |  | RO | Num | ND | NC | PT |
11.093 | Additional Identifier Characters 3 | -2147483648 to 2147483647 |  | RO | Num | ND | NC | PT |
11.094 | Disable String Mode | Off (0) or On (1) | Off (0) | RW | Bit |  |  | PT | US
11.097 | AI ID Code | None (0), Sd.Card (1), RS‑485 (2), Res (3), Res (4), 485.24V (5) |  | RO | Txt | ND | NC | PT |
11.098 | 24V Loss Alarm Enable | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
11.099 | Modbus Parameter Conversion | 0000 to 1111 | 0000 | RW | Bin |  |  |  | US

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |