# Menu 40 Single Line Descriptions − AMC Homing System

Mode: RFC‑S

Parameter | Range | Default | Type
--- | --- | --- | ---
40.001 | AMC Home Direction | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
40.002 | AMC Home Mode | 0 to 8 | 0 | RW | Num |  |  |  | US
40.003 | AMC Home Maximum Speed | ±VM_AMC_SPEED_UNIPOLAR UU/ms | 10.92 UU/ms | RW | Num |  |  |  | US
40.004 | AMC Home Position | ±VM_AMC_POSITION UU | 0 UU | RW | Num |  |  |  | US
40.005 | AMC Home Complete | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
40.006 | AMC Home Offset Maximum Speed | ±VM_AMC_SPEED_UNIPOLAR UU/ms | 10.92 UU/ms | RW | Num |  |  |  | US
40.007 | AMC Home Offset Position | ±VM_AMC_POSITION UU | 0 UU | RW | Num |  |  |  | US
40.008 | AMC Home Offset Complete | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
40.009 | AMC Home Maximum Allowed Move | 0 to VM_AMC_POSITION_UNIPOLAR UU | 0 UU | RW | Num |  |  |  | US
40.010 | AMC Home Complete Window | 0 to VM_AMC_POSITION_UNIPOLAR UU | 0 UU | RW | Num |  |  |  | US
40.011 | AMC Home On Freeze | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
40.012 | AMC Home Switch | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
40.013 | AMC Home Positive Limit | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
40.014 | AMC Home Negative Limit | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |
40.015 | AMC Home Positive Limit Selector | 0 to 2 | 0 | RW | Num |  |  |  | US
40.016 | AMC Home Negative Limit Selector | 0 to 2 | 0 | RW | Num |  |  |  | US
40.017 | AMC Home Torque Limit Active | Off (0) or On (1) |  | RO | Bit | ND | NC | PT |
40.018 | AMC Home Hard Stop Torque Threshold | 0.0 to 1000.0 % | 0.0 % | RW | Num |  |  |  | US
40.019 | AMC Home Hard Stop Delay Time | 0.000 to 60.000 s | 0.000 s | RW | Num |  |  |  | US
40.020 | AMC Home Required | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
40.021 | AMC Home Slave Source | None (-1), User Position (0), Sensorless (1), P1 Drive (2), P2 Drive (3), P1 Slot1 (4), P2 Slot1 (5), P1 Slot2 (6), P2 Slot3 (9) | None (-1) | RW | Txt |  |  |  | US

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |