# Menu 32 Single Line Descriptions − AMC Master Position

Mode: RFC‑S

Parameter | Range | Default | Type
--- | --- | --- | ---
32.001 | AMC Master Source Select | Speed (0), User Position (1), P1 Drive (2), P2 Drive (3), P1 Slot1 (4), P2 Slot1 (5), P1 Slot2 (6), P2 Slot2 (7) | P2 Drive (3) | RW | Txt |  |  |  | US
32.002 | AMC Master Invert | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
32.003 | AMC Master Offset | ±VM_AMC_POSITION UU | 0 UU | RW | Num |  |  |  | US
32.004 | AMC Master Position | ±VM_AMC_POSITION UU |  | RO | Num | ND | NC | PT |
32.005 | AMC Master Speed | ±VM_AMC_SPEED UU/ms |  | RO | Num | ND | NC | PT | FI
32.006 | AMC Master Freeze Position | ±VM_AMC_POSITION UU |  | RO | Num | ND | NC | PT |
32.007 | AMC Master Freeze Select | Off (0) or On (1) | Off (0) | RW | Bit |  |  |  | US
32.008 | AMC Master Speed Reference | ±VM_AMC_SPEED UU/ms | 0.00 UU/ms | RW | Num |  |  |  | US
32.009 | AMC Master User Position Reference | -2147483648 to 2147483647 | 0 | RW | Num |  | NC |  |
32.010 | AMC Master Freeze Flag | Off (0) or On (1) | Off (0) | RW | Bit |  | NC |  |

RW | Read / Write | RO | Read-only | Bit | Bit parameter | Txt | Text string | Date | Date parameter | Time | Time parameter
Chr | Character parameter | Bin | Binary parameter | IP | IP address | Mac | MAC address | Ver | Version number | SMP | Slot, menu, parameter
Num | Number parameter | DE | Destination | ND | No default value | RA | Rating dependent | NC | Non-copyable | PT | Protected
FI | Filtered | US | User save | PS | Power-down save |  |  |  |  |  |